Pro 24DSP:
-Introduced an updated VRM GUI, now with head rotation and direction indicators. 

Liquid Saffire 56:
-The SPDIF Outputs on the Liquid Saffire 56 can now be switched to the AES/EBU standard operating level. 
-The transformer loading on the Liquid preamps could cause some level problems with certain microphones. There is now a per channel option in the settings menu to switch this loading off.

All devices:
-Clickable menus made clearer by arrow icons
-Included some bug fixes related to dual device naming and snapshot loading
-Fixed an issue installing Saffire MixControl under a certain types of user account (Mac OS X 10.4 and 10.5)